{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":2,"defined_names":0,"comments":3,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":41,"n_cols":23,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Rs",435,null,"базовая длина анкеровки, ds:",{"$nulls":6},"базовая длина анкеровки, мм:",{"$nulls":7},"анкеровка:",null,">15d",180]
["d",12,null,"анкеровка растянутых стержней, ds (Ns = Rs):",{"$nulls":6},"анкеровка растянутых стержней, мм (Ns = Rs):",{"$nulls":9},">200мм",200,200]
["As",1.1309733552923256,null,"α=1,0","B20","B25","B30","B35","B40",null,"α=1,0","B20","B25","B30","B35","B40"]
[null,null,null,"В500С",58,50,45,40,37,null,"В500С",700,600,540,480,440]
["us",3.7699111843077517,null,"А240, А400",40,34,31,28,26,null,"А240, А400",480,410,370,340,310,null,null,"нахлёст: ",null,">20d",240]
["n1",2.5,null,"А500С",49,42,38,34,32,null,"А500С",590,500,460,410,380,{"$nulls":4},">250мм",250,250]
["n2",1,null,"А500СП",45,39,35,31,29,null,"А500СП",540,470,420,370,350]
["Rbt",1.15]
["Rbond",2.875,null,"анкеровка сжатых стержней, ds (Ns = Rs):",{"$nulls":6},"анкеровка сжатых стержней, мм (Ns = Rs):",{"$nulls":6},"анкеровка стержней, мм (Ns = 30% Rs):"]
[null,null,null,"α=0,75","B20","B25","B30","B35","B40",null,"α=0,75","B20","B25","B30","B35","B40",null,"α=0,3","B20","B25","B30","B35","B40"]
[null,null,null,"В500С",44,38,34,30,28,null,"В500С",530,450,410,360,330,null,"В500С",210,200,200,200,200]
["l0=",45.39130434782609,"см","А240, А400",30,26,24,21,20,null,"А240, А400",360,310,280,260,230,null,"А240, А400",200,200,200,200,200]
["l0=",37.82608695652174,"ds","А500С",37,32,29,26,24,null,"А500С",440,380,350,310,290,null,"А500С",200,200,200,200,200]
[null,null,null,"А500СП",34,30,27,24,22,null,"А500СП",410,350,320,280,260,null,"А500СП",200,200,200,200,200]
[]
[null,null,null,"нахлёст растянутых стержней, ds (Ns = Rs):",{"$nulls":6},"нахлёст растянутых стержней, мм (Ns = Rs):",{"$nulls":6},"нахлёст растянутых стержней, мм (Ns = 40% Rs):"]
[null,null,null,"α=1,2","B20","B25","B30","B35","B40",null,"α=1,2","B20","B25","B30","B35","B40",null,"α=1,2*0,4","B20","B25","B30","B35","B40"]
[null,null,null,"В500С",70,60,54,48,45,null,"В500С",840,720,650,580,530,null,"В500С",340,290,260,250,250]
[null,null,null,"А240, А400",48,41,38,34,32,null,"А240, А400",580,490,440,410,370,null,"А240, А400",250,250,250,250,250]
[null,null,null,"А500С",59,51,46,41,39,null,"А500С",710,600,550,490,460,null,"А500С",280,250,250,250,250]
[null,null,null,"А500СП",54,47,42,38,35,null,"А500СП",650,560,500,440,420,null,"А500СП",260,250,250,250,250]
[]
[null,null,null,"нахлёст сжатых стержней, ds (Ns = Rs):",{"$nulls":6},"нахлёст сжатых стержней, мм (Ns = Rs):",{"$nulls":6},"нахлёст сжатых стержней, мм (Ns = 40% Rs):"]
[null,null,null,"α=0,9","B20","B25","B30","B35","B40",null,"α=0,9","B20","B25","B30","B35","B40",null,"α=0,9*0,4","B20","B25","B30","B35","B40"]
[null,null,null,"В500С",53,45,41,36,34,null,"В500С",630,540,490,430,400,null,"В500С",250,250,250,250,250]
[null,null,null,"А240, А400",36,31,28,26,24,null,"А240, А400",430,370,330,310,280,null,"А240, А400",250,250,250,250,250]
[null,null,null,"А500С",45,38,35,31,29,null,"А500С",530,450,410,370,340,null,"А500С",250,250,250,250,250]
[null,null,null,"А500СП",41,36,32,28,27,null,"А500СП",490,420,380,330,320,null,"А500СП",250,250,250,250,250]
[]
[null,null,null,"нахлёст сжатых стержней, ds (Ns = Rs):",{"$nulls":6},"нахлёст сжатых стержней, мм (Ns = Rs):"]
[null,null,null,"доп. приварка поперечной арматуры",{"$nulls":6},"доп. приварка поперечной арматуры"]
[null,null,null,"α=0,9*0,7","B20","B25","B30","B35","B40",null,"α=0,9*0,7","B20","B25","B30","B35","B40"]
[null,null,null,"В500С",37,32,29,26,24,null,"В500С",440,380,340,300,280]
[null,null,null,"А240, А400",26,22,20,18,17,null,"А240, А400",300,260,250,250,250]
[null,null,null,"А500С",31,27,24,22,21,null,"А500С",370,320,290,260,250]
[null,null,null,"А500СП",29,25,23,20,19,null,"А500СП",340,300,260,250,250]
[]
[]
["Расчёт по СП 52-101-2003"]
["п.8.3.21, 8.3.22, 8.3.27"]
["http://fordewind.org/"]